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The loudspeaker shall contain a two-way, 12-inch coaxially mounted woofer and a center-firing 1.4-inch compression driver.
The loudspeaker shall meet the following performance specifications: On-axis system frequency range shall be 38 Hz to 20 kHz (-10 dB) with the use of recommended active equalization. The loudspeaker sensitivity shall be 94 dB SPL in whole-space environment with recommended high-pass protection with 1 W input at 1 meter. The long-term power handling rating shall be 300 W (AES test methodology using IEC system noise, 2-hour duration). Maximum continuous output shall be 119 dB SPL and the maximum peak output shall be 125 dB SPL. The nominal coverage pattern shall be 102° conical at 500 Hz – 8 kHz.
The loudspeaker shall be constructed of an engineered-plastics, UV fade-resistant enclosure. The loudspeaker shall consist of PC-ABS plastic materials that are resilient to cooking oil exposure. The loudspeaker shall be ETL- and cETL-certified under UL 1480A & CSA 22.2 No. 205-17. The transducers shall be located behind a perforated aluminum grille with a powder-coated finish that is magnetically attached with a tamper-resistant design. The loudspeaker shall contain a pan-and-tilt bracket mounting system. The loudspeaker shall be suitable for use outdoors, with an ingress rating of IP55. The loudspeaker shall be available in black or white and shall be paintable. Input connectors shall be a 4-pin Euroblock connector. The loudspeaker shall have a nominal rated impedance of 8 ohms. The loudspeaker dimensions shall be 485 × 407 × 406 mm (19.1 × 16.0 × 16.0 in) and net weight shall be 16.9 kg (37.4 lb).
The warranty shall be 5 years. 
The loudspeaker shall be the DesignMax DM12SE surface-mounted loudspeaker.

